Supported ENVISAT Products |

## Scan and pixel number nadir view ADS

Fields of ENVISAT ATS_TOA_1P_ADSR_pix Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"dsr_time"` | MJD | 1 | Nadir UTC time in MJD format | MJD
1 | `"attach_flag"` | UChar | 1 | Attachment flag (always set to zero for this ADS) | flag
2 | `"spare_1"` | Spare | 1 | Spare | -
3 | `"img_scan_y"` | SLong | 1 | image scan y coordinate | m
4 | `"instr_scan_num"` | UShort | 512 | instrument scan number | -
5 | `"pix_num"` | UShort | 512 | pixel number | -