Create DEM-related Bands |

### Create DEM-related Bands

This command adds a new DEM-elevation band and optionally DEM-corrected latitude and longitude bands to the current product. The bands are computed by looking up each pixel in a selected high-resolution DEM (which is by default GETASSE30). As opposed to the orthorectification tool, which always reprojects the data product, the DEM-corrected latitudes and longitudes are computed in the selected product's current coordinate system.

- Digital elevation model (DEM)
  Lets you select a DEM from the list of currently installed DEMs.
- Elevation band name
  The name of the new elevation band.
- Output DEM-corrected bands
  Check if DEM-corrected bands shall be created. Depending on the data product type, this option may not be available.
- Latitude band name
  The name of the new DEM-corrected latitude band.
- Longitude band name
  The name of the new DEM-corrected longitude band.