Supported ENVISAT Products |

INDEX PRODUCTS FLAGS

## AATSR Gridded brightness temperature and reflectance

Bands of ENVISAT ATS_TOA_1P Products

Tie-Point Grids of ENVISAT

Index | Identifier | Type | Description | Units | Bitmask
0 | `"latitude"` | Float | Latitudes | deg | n/a
1 | `"longitude"` | Float | Longitudes | deg | n/a
2 | `"lat_corr_nadir"` | Float | Latitude corrections, nadir view | deg | n/a
3 | `"lon_corr_nadir"` | Float | Longitude corrections, nadir view | deg | n/a
4 | `"lat_corr_fward"` | Float | Latitude corrections, forward view | deg | n/a
5 | `"lon_corr_fward"` | Float | Longitude corrections, forward view | deg | n/a
6 | `"altitude"` | Float | Topographic altitude | m | n/a
7 | `"sun_elev_nadir"` | Float | Solar elevation, nadir view | deg | n/a
8 | `"view_elev_nadir"` | Float | Satellite elevation, nadir view | deg | n/a
9 | `"sun_azimuth_nadir"` | Float | Solar azimuth, nadir view | deg | n/a
10 | `"view_azimuth_nadir"` | Float | Satellite azimuth, nadir view | deg | n/a
11 | `"sun_elev_fward"` | Float | Solar elevation, forward view | deg | n/a
12 | `"view_elev_fward"` | Float | Satellite elevation, forward view | deg | n/a
13 | `"sun_azimuth_fward"` | Float | Solar azimuth, forward view | deg | n/a
14 | `"view_azimuth_fward"` | Float | Satellite azimuth, forward view | deg | n/a

Bands of ENVISAT

Index | Identifier | Type | Description | Units | Bitmask
15 | `"btemp_nadir_1200"` | Float | Brightness temperature, nadir view (11500-12500 nm) | K | n/a
16 | `"btemp_nadir_1100"` | Float | Brightness temperature, nadir view (10400-11300 nm) | K | n/a
17 | `"btemp_nadir_0370"` | Float | Brightness temperature, nadir view (3505-3895 nm) | K | n/a
18 | `"reflec_nadir_1600"` | Float | Refectance, nadir view (1580-1640 nm) | % | n/a
19 | `"reflec_nadir_0870"` | Float | Refectance, nadir view (855-875 nm) | % | n/a
20 | `"reflec_nadir_0670"` | Float | Refectance, nadir view (649-669 nm) | % | n/a
21 | `"reflec_nadir_0550"` | Float | Refectance, nadir view (545-565 nm) | % | n/a
22 | `"btemp_fward_1200"` | Float | Brightness temperature, forward view (11500-12500 nm) | K | n/a
23 | `"btemp_fward_1100"` | Float | Brightness temperature, forward view (10400-11300 nm) | K | n/a
24 | `"btemp_fward_0370"` | Float | Brightness temperature, forward view (3505-3895 nm) | K | n/a
25 | `"reflec_fward_1600"` | Float | Refectance, forward view (1580-1640 nm) | % | n/a
26 | `"reflec_fward_0870"` | Float | Refectance, forward view (855-875 nm) | % | n/a
27 | `"reflec_fward_0670"` | Float | Refectance, forward view (649-669 nm) | % | n/a
28 | `"reflec_fward_0550"` | Float | Refectance, forward view (545-565 nm) | % | n/a
29 | `"confid_flags_nadir"` | UShort | Confidence flags, nadir view | n/a | n/a
30 | `"confid_flags_fward"` | UShort | Confidence flags, forward view | n/a | n/a
31 | `"cloud_flags_nadir"` | UShort | Cloud flags, nadir view | n/a | n/a
32 | `"cloud_flags_fward"` | UShort | Cloud flags, forward view | n/a | n/a