Supported ENVISAT Products |

## Wave Mode processing parameters

Fields of ENVISAT ASAR_Wave_Param_ADSR Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"first_zero_doppler_time"` | MJD | 1 | First Zero Doppler Azimuth time of MDS which this data set describesTime of first range line in the MDS described by this data set | MJD
1 | `"attach_flag"` | UChar | 1 | Attachment Flag (always set to zero for this ADSR) | flag
2 | `"last_zero_doppler_time"` | MJD | 1 | Last Zero Doppler Azimuth time of MDS which this data set describesTime of last range line in the MDS described by this data set | MJD
3 | `"work_order_id"` | String | 1 | Work Order ID (left-justified) | ascii
4 | `"time_diff"` | Float | 1 | Time difference between sensing time of first input line and zero Doppler time of first output image line (tdelta). (TBC)May be used during child product extraction from a stripline product (TBC). Left blank (set to zero) for non-stripline products | s
5 | `"swath_id"` | String | 1 | Swath number IS1, IS2, IS3, IS4, IS5, IS6, or IS7 for IM, WV and AP modes.Set to WSØ for WS and GM modes | ascii
6 | `"range_spacing"` | Float | 1 | Range sample spacing | m
7 | `"azimuth_spacing"` | Float | 1 | Azimuth sample spacing at image center | m
8 | `"line_time_interval"` | Float | 1 | Azimuth sample spacing in time (Line Time Interval) | s
9 | `"num_output_lines"` | ULong | 1 | Number of output range lines in the image described by this ADS | lines
10 | `"num_samples_per_line"` | ULong | 1 | Number of samples per output range line (includes zero filled samples) | samples
11 | `"data_type"` | String | 1 | Output data typeSWORD, UWORD, or UBYTE | ascii
12 | `"spare_1"` | Spare | 1 | Spare | -
13 | `"data_analysis_flag"` | UChar | 1 | Raw Data Analysis used for Raw Data Correction 0 = correction done using default parameters1 = correction done using raw data analysis results | flag
14 | `"ant_elev_corr_flag"` | UChar | 1 | Antenna Elevation Pattern Correction Applied 0 = no correction applied1 = correction applied | flag
15 | `"chirp_extract_flag"` | UChar | 1 | reconstructed Chirp used 0 = nominal chirp replica used1 = reconstructed chirp used | flag
16 | `"srgr_flag"` | UChar | 1 | Slant Range to Ground Range Conversion Applied0 = no conversion applied1 = conversion applied | flag
17 | `"dop_cen_flag"` | UChar | 1 | Doppler Centroid Estimation Performed0 = no estimation done1 = estimation done | flag
18 | `"dop_amb_flag"` | UChar | 1 | Doppler Ambiguity Estimation Performed0 = no estimate done1 = estimate done | flag
19 | `"range_spread_comp_flag"` | UChar | 1 | Range-spreading loss compensation Applied0 = no compensation applied1 = compensation applied | flag
20 | `"detected_flag"` | UChar | 1 | Detection Applied0 = output product is complex1 = output product was detected | flag
21 | `"look_sum_flag"` | UChar | 1 | Look Summation Performed0 = product is single look1 = product is multi-looked | flag
22 | `"rms_equal_flag"` | UChar | 1 | RMS Equalization performed 0= rms equalization not performed during FBAQ decoding, 1 = rms equalization performed during FBAQ decoding | flag
23 | `"ant_scal_flag"` | UChar | 1 | Antenna Elevationscaling Factor applied 0= no scaling factor applied, 1 = scaling factor applied | flag
24 | `"spare_2"` | Spare | 1 | Spare | -
25 | `"raw_data_analysis.1.num_gaps"` | ULong | 1 | Number of input data gaps (a gap is defined as a predetermined number of range lines) (record 1) | gaps
26 | `"raw_data_analysis.1.num_missing_lines"` | ULong | 1 | Number of missing lines, excluding data gaps (record 1) | lines
27 | `"raw_data_analysis.1.range_samp_skip"` | ULong | 1 | Range sample skipping factor for raw data analysis (record 1) | samples
28 | `"raw_data_analysis.1.range_lines_skip"` | ULong | 1 | Range lines skipping factor for raw data analysis (record 1) | lines
29 | `"raw_data_analysis.1.calc_i_bias"` | Float | 1 | Calculated I channel bias (record 1) | -
30 | `"raw_data_analysis.1.calc_q_bias"` | Float | 1 | Calculated Q channel bias (record 1) | -
31 | `"raw_data_analysis.1.calc_i_std_dev"` | Float | 1 | Calculated I channel standard deviation (record 1) | -
32 | `"raw_data_analysis.1.calc_q_std_dev"` | Float | 1 | Calculated Q channel standard deviation (record 1) | -
33 | `"raw_data_analysis.1.calc_gain"` | Float | 1 | Calculated I/Q gain imbalance (record 1) | -
34 | `"raw_data_analysis.1.calc_quad"` | Float | 1 | Calculated I/Q quadrature departure (record 1) | -
35 | `"raw_data_analysis.1.i_bias_max"` | Float | 1 | I bias upper bound (record 1) | -
36 | `"raw_data_analysis.1.i_bias_min"` | Float | 1 | I bias lower bound (record 1) | -
37 | `"raw_data_analysis.1.q_bias_max"` | Float | 1 | Q bias upper bound (record 1) | -
38 | `"raw_data_analysis.1.q_bias_min"` | Float | 1 | Q bias lower bound (record 1) | -
39 | `"raw_data_analysis.1.gain_min"` | Float | 1 | I/Q gain lower bound (record 1) | -
40 | `"raw_data_analysis.1.gain_max"` | Float | 1 | I/Q gain upper bound (record 1) | -
41 | `"raw_data_analysis.1.quad_min"` | Float | 1 | I/Q quadrature departure lower bound (record 1) | -
42 | `"raw_data_analysis.1.quad_max"` | Float | 1 | I/Q quadrature departure upper bound (record 1) | -
43 | `"raw_data_analysis.1.i_bias_flag"` | UChar | 1 | I bias significance0 = I bias falls within acceptable range1 = I bias falls outside acceptable range (record 1) | flag
44 | `"raw_data_analysis.1.q_bias_flag"` | UChar | 1 | Q bias Significance0 = Q bias falls within acceptable range1 = Q bias falls outside acceptable range (record 1) | flag
45 | `"raw_data_analysis.1.gain_flag"` | UChar | 1 | I/Q Gain Significance0 = Gain falls within acceptable range1 = Gain falls outside acceptable range (record 1) | flag
46 | `"raw_data_analysis.1.quad_flag"` | UChar | 1 | I/Q Quadrature Departure Significance0 = Quadrature departure falls within acceptable range1 =Quadrature departure falls outside acceptable range (record 1) | flag
47 | `"raw_data_analysis.1.used_i_bias"` | Float | 1 | I channel bias used for correction (may be different from measured value) (record 1) | -
48 | `"raw_data_analysis.1.used_q_bias"` | Float | 1 | Q channel bias used for correction(may be different from measured value) (record 1) | -
49 | `"raw_data_analysis.1.used_gain"` | Float | 1 | I/Q gain imbalance used for correction(may be different from measured value) (record 1) | -
50 | `"raw_data_analysis.1.used_quad"` | Float | 1 | I/Q quadrature departure used for correction(may be different from measured value) (record 1) | -
51 | `"raw_data_analysis.2.num_gaps"` | ULong | 1 | Number of input data gaps (a gap is defined as a predetermined number of range lines) (record 2) | gaps
52 | `"raw_data_analysis.2.num_missing_lines"` | ULong | 1 | Number of missing lines, excluding data gaps (record 2) | lines
53 | `"raw_data_analysis.2.range_samp_skip"` | ULong | 1 | Range sample skipping factor for raw data analysis (record 2) | samples
54 | `"raw_data_analysis.2.range_lines_skip"` | ULong | 1 | Range lines skipping factor for raw data analysis (record 2) | lines
55 | `"raw_data_analysis.2.calc_i_bias"` | Float | 1 | Calculated I channel bias (record 2) | -
56 | `"raw_data_analysis.2.calc_q_bias"` | Float | 1 | Calculated Q channel bias (record 2) | -
57 | `"raw_data_analysis.2.calc_i_std_dev"` | Float | 1 | Calculated I channel standard deviation (record 2) | -
58 | `"raw_data_analysis.2.calc_q_std_dev"` | Float | 1 | Calculated Q channel standard deviation (record 2) | -
59 | `"raw_data_analysis.2.calc_gain"` | Float | 1 | Calculated I/Q gain imbalance (record 2) | -
60 | `"raw_data_analysis.2.calc_quad"` | Float | 1 | Calculated I/Q quadrature departure (record 2) | -
61 | `"raw_data_analysis.2.i_bias_max"` | Float | 1 | I bias upper bound (record 2) | -
62 | `"raw_data_analysis.2.i_bias_min"` | Float | 1 | I bias lower bound (record 2) | -
63 | `"raw_data_analysis.2.q_bias_max"` | Float | 1 | Q bias upper bound (record 2) | -
64 | `"raw_data_analysis.2.q_bias_min"` | Float | 1 | Q bias lower bound (record 2) | -
65 | `"raw_data_analysis.2.gain_min"` | Float | 1 | I/Q gain lower bound (record 2) | -
66 | `"raw_data_analysis.2.gain_max"` | Float | 1 | I/Q gain upper bound (record 2) | -
67 | `"raw_data_analysis.2.quad_min"` | Float | 1 | I/Q quadrature departure lower bound (record 2) | -
68 | `"raw_data_analysis.2.quad_max"` | Float | 1 | I/Q quadrature departure upper bound (record 2) | -
69 | `"raw_data_analysis.2.i_bias_flag"` | UChar | 1 | I bias significance0 = I bias falls within acceptable range1 = I bias falls outside acceptable range (record 2) | flag
70 | `"raw_data_analysis.2.q_bias_flag"` | UChar | 1 | Q bias Significance0 = Q bias falls within acceptable range1 = Q bias falls outside acceptable range (record 2) | flag
71 | `"raw_data_analysis.2.gain_flag"` | UChar | 1 | I/Q Gain Significance0 = Gain falls within acceptable range1 = Gain falls outside acceptable range (record 2) | flag
72 | `"raw_data_analysis.2.quad_flag"` | UChar | 1 | I/Q Quadrature Departure Significance0 = Quadrature departure falls within acceptable range1 =Quadrature departure falls outside acceptable range (record 2) | flag
73 | `"raw_data_analysis.2.used_i_bias"` | Float | 1 | I channel bias used for correction (may be different from measured value) (record 2) | -
74 | `"raw_data_analysis.2.used_q_bias"` | Float | 1 | Q channel bias used for correction(may be different from measured value) (record 2) | -
75 | `"raw_data_analysis.2.used_gain"` | Float | 1 | I/Q gain imbalance used for correction(may be different from measured value) (record 2) | -
76 | `"raw_data_analysis.2.used_quad"` | Float | 1 | I/Q quadrature departure used for correction(may be different from measured value) (record 2) | -
77 | `"spare_3"` | Spare | 1 | Spare | -
78 | `"start_time.1.first_obt"` | ULong | 2 | On-board binary time of first input line processedLSB accurate to 15.26 ms. (Contained in two long integers) (record 1) | -
79 | `"start_time.1.first_mjd"` | MJD | 1 | Sensing time (MJD format) of first input line processedconverted from satellite binary time (record 1) | MJD
80 | `"start_time.2.first_obt"` | ULong | 2 | On-board binary time of first input line processedLSB accurate to 15.26 ms. (Contained in two long integers) (record 2) | -
81 | `"start_time.2.first_mjd"` | MJD | 1 | Sensing time (MJD format) of first input line processedconverted from satellite binary time (record 2) | MJD
82 | `"parameter_codes.swst_code"` | UShort | 5 | Sampling Window Start time code of first processed line | code
83 | `"parameter_codes.last_swst_code"` | UShort | 5 | Sampling Window Start time code of last processed line | code
84 | `"parameter_codes.pri_code"` | UShort | 5 | Pulse Repetition Interval code | code
85 | `"parameter_codes.tx_pulse_len_code"` | UShort | 5 | Tx pulse length | code
86 | `"parameter_codes.tx_bw_code"` | UShort | 5 | Tx pulse bandwidth | code
87 | `"parameter_codes.echo_win_len_code"` | UShort | 5 | Echo Window Length | code
88 | `"parameter_codes.up_code"` | UShort | 5 | Upconverter Level - Upconverter gain set on the instrument | code
89 | `"parameter_codes.down_code"` | UShort | 5 | Downconverter Level - Downconverter gain set on the instrument | code
90 | `"parameter_codes.resamp_code"` | UShort | 5 | Resampling factor for echo data | code
91 | `"parameter_codes.beam_adj_code"` | UShort | 5 | Beam adjustment delta | code
92 | `"parameter_codes.beam_set_num_code"` | UShort | 5 | Antenna Beam Set Number | code
93 | `"parameter_codes.tx_monitor_code"` | UShort | 5 | Auxiliary Tx Monitor Level | code
94 | `"spare_4"` | Spare | 1 | Spare | -
95 | `"error_counters.num_err_swst"` | ULong | 1 | Number of errors detected in Sampling Window start time field. | -
96 | `"error_counters.num_err_pri"` | ULong | 1 | Number of errors detected in PRI code field | -
97 | `"error_counters.num_err_tx_pulse_len"` | ULong | 1 | Number of errors detected in Tx pulse length field | -
98 | `"error_counters.num_err_tx_pulse_bw"` | ULong | 1 | Number of errors detected in Tx pulse bandwidth field. | -
99 | `"error_counters.num_err_echo_win_len"` | ULong | 1 | Number of errors detected in Echo Window Length field. | -
100 | `"error_counters.num_err_up"` | ULong | 1 | Number of errors detected in Upconverter Level field. | -
101 | `"error_counters.num_err_down"` | ULong | 1 | Number of errors detected in Downconverter Level field. | -
102 | `"error_counters.num_err_resamp"` | ULong | 1 | Number of errors detected in Resampling factor for echo data field. | -
103 | `"error_counters.num_err_beam_adj"` | ULong | 1 | Number of errors detected in Beam adjustment delta field. | -
104 | `"error_counters.num_err_beam_set_num"` | ULong | 1 | Number of errors detected in Antenna Beam Set Number field. | -
105 | `"spare_5"` | Spare | 1 | Spare | -
106 | `"image_parameters.swst_value"` | Float | 5 | Sampling Window Start time of first processed line | s
107 | `"image_parameters.last_swst_value"` | Float | 5 | Sampling Window Start time of last processed line | s
108 | `"image_parameters.swst_changes"` | ULong | 5 | Number of Sample Window Start Time changes within a beam | -
109 | `"image_parameters.prf_value"` | Float | 5 | Pulse Repetition Frequency | Hz
110 | `"image_parameters.tx_pulse_len_value"` | Float | 5 | Tx pulse length | s
111 | `"image_parameters.tx_pulse_bw_value"` | Float | 5 | Tx pulse bandwidth | Hz
112 | `"image_parameters.echo_win_len_value"` | Float | 5 | Echo Window Length | s
113 | `"image_parameters.up_value"` | Float | 5 | Upconverter Level - Upconverter gain set on the instrument | dB
114 | `"image_parameters.down_value"` | Float | 5 | Downconverter Level - Downconverter gain set on the instrument | dB
115 | `"image_parameters.resamp_value"` | Float | 5 | Resampling factor | -
116 | `"image_parameters.beam_adj_value"` | Float | 5 | Beam adjustment delta | deg.
117 | `"image_parameters.beam_set_value"` | UShort | 5 | Antenna Beam Set Number | -
118 | `"image_parameters.tx_monitor_value"` | Float | 5 | Auxiliary Tx Monitor Level | -
119 | `"spare_6"` | Spare | 1 | Spare | -
120 | `"first_proc_range_samp"` | ULong | 1 | First processed input range sample, first sample is 1 | samples
121 | `"range_ref"` | Float | 1 | Range spreading loss reference range | m
122 | `"range_samp_rate"` | Float | 1 | Range sampling rate | Hz
123 | `"radar_freq"` | Float | 1 | Radar Frequency | Hz
124 | `"num_looks_range"` | UShort | 1 | Number of range looks | looks
125 | `"filter_range"` | String | 1 | Matched filter window type:HAMMING or KAISERØ or NONEØØØ | ascii
126 | `"filter_coef_range"` | Float | 1 | Window coefficient for range-matched filter | -
127 | `"bandwidth.look_bw_range"` | Float | 5 | Range Look Bandwidth (null to null) | Hz
128 | `"bandwidth.tot_bw_range"` | Float | 5 | Total processed range bandwidth (null to null) | Hz
129 | `"nominal_chirp.1.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 1) | -, s-1, s-2, s-3
130 | `"nominal_chirp.1.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 1) | cycles,Hz,Hz/s,Hz/s2
131 | `"nominal_chirp.2.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 2) | -, s-1, s-2, s-3
132 | `"nominal_chirp.2.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 2) | cycles,Hz,Hz/s,Hz/s2
133 | `"nominal_chirp.3.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 3) | -, s-1, s-2, s-3
134 | `"nominal_chirp.3.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 3) | cycles,Hz,Hz/s,Hz/s2
135 | `"nominal_chirp.4.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 4) | -, s-1, s-2, s-3
136 | `"nominal_chirp.4.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 4) | cycles,Hz,Hz/s,Hz/s2
137 | `"nominal_chirp.5.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 5) | -, s-1, s-2, s-3
138 | `"nominal_chirp.5.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 5) | cycles,Hz,Hz/s,Hz/s2
139 | `"spare_7"` | Spare | 1 | Spare | -
140 | `"num_lines_proc"` | ULong | 1 | Number of input lines processed | lines
141 | `"num_look_az"` | UShort | 1 | Number of Azimuth Looks | looks
142 | `"look_bw_az"` | Float | 1 | Azimuth Look Bandwidth (null to null) -- this is the nominal value only for GM, WS, and AP. | Hz
143 | `"to_bw_az"` | Float | 1 | Processed Azimuth bandwidth (null to null) -- this field is used only for IM products and WV imagettes. Filled with zeros otherwise. | Hz
144 | `"filter_az"` | String | 1 | Matched filter window type:HAMMING or KAISERØ or NONEØØØ | ascii
145 | `"filter_coef_az"` | Float | 1 | Window coefficient for azimuth-matched filter | -
146 | `"az_fm_rate"` | Float | 3 | 3 co-efficients for Azimuth FM rate:Azimuth FM rate = C0 + C1(tSR-t0) + C2(tSR - t0)2tSR = 2 way slant range time | Hz/sHz/s2Hz/s3
147 | `"ax_fm_origin"` | Float | 1 | 2 way slant range time origin (t0) for Azimuth FM rate calculation | ns
148 | `"dop_amb_conf"` | Float | 1 | Doppler Centroid Ambiguity Confidence MeasureValue between 0 and 1, 0 = poorest confidence, 1= highest confidence | -
149 | `"spare_8"` | Spare | 1 | Spare | -
150 | `"calibration_factors.1.proc_scaling_fact"` | Float | 1 | Processor scaling factor (record 1) | -
151 | `"calibration_factors.1.ext_cal_fact"` | Float | 1 | External Calibration Scaling Factor (mode/swath/polarization dependent) (record 1) | -
152 | `"calibration_factors.2.proc_scaling_fact"` | Float | 1 | Processor scaling factor (record 2) | -
153 | `"calibration_factors.2.ext_cal_fact"` | Float | 1 | External Calibration Scaling Factor (mode/swath/polarization dependent) (record 2) | -
154 | `"noise_estimation.noise_power_corr"` | Float | 5 | Noise power correction factors | -
155 | `"noise_estimation.num_noise_lines"` | ULong | 5 | Number of noise lines used to calculate factors | -
156 | `"spare_9"` | Spare | 1 | Spare | -
157 | `"spare_10"` | Spare | 1 | Spare | -
158 | `"output_statistics.1.out_mean"` | Float | 1 | Output data mean Magnitude for detected products, real sample mean for SLC products (record 1) | -
159 | `"output_statistics.1.out_imag_mean"` | Float | 1 | Output imaginary data mean Used for SLC products only (set to zero otherwise) (record 1) | -
160 | `"output_statistics.1.out_std_dev"` | Float | 1 | Output data standard deviation Magnitude std. dev. for detected products, real sample std. dev. for SLC products (record 1) | -
161 | `"output_statistics.1.out_imag_std_dev"` | Float | 1 | Output imaginary data standard deviation Used for SLC products only (set to zero otherwise) (record 1) | -
162 | `"output_statistics.2.out_mean"` | Float | 1 | Output data mean Magnitude for detected products, real sample mean for SLC products (record 2) | -
163 | `"output_statistics.2.out_imag_mean"` | Float | 1 | Output imaginary data mean Used for SLC products only (set to zero otherwise) (record 2) | -
164 | `"output_statistics.2.out_std_dev"` | Float | 1 | Output data standard deviation Magnitude std. dev. for detected products, real sample std. dev. for SLC products (record 2) | -
165 | `"output_statistics.2.out_imag_std_dev"` | Float | 1 | Output imaginary data standard deviation Used for SLC products only (set to zero otherwise) (record 2) | -
166 | `"spare_11"` | Spare | 1 | Spare | -
167 | `"echo_comp"` | String | 1 | Compression Method used for echo samples FBAQ, S&MØ, NONE | ascii
168 | `"echo_comp_ratio"` | String | 1 | Compression Ratio for echo samples8/4, 8/3, 8/2, or 8/8 | ascii
169 | `"init_cal_comp"` | String | 1 | Compression Method used for initial calibration samples FBAQ, S&MØ, NONE | ascii
170 | `"init_cal_ratio"` | String | 1 | Compression Ratio for initial calibration samples8/4, 8/3, 8/2, or 8/8 | ascii
171 | `"per_cal_comp"` | String | 1 | Compression Method used for periodic calibration samples FBAQ, S&MØ, NONE | ascii
172 | `"per_cal_ratio"` | String | 1 | Compression Ratio for periodic calibration samples8/4, 8/3, 8/2, or 8/8 | ascii
173 | `"noise_comp"` | String | 1 | Compression Method used for noise samples FBAQ, S&MØ, NONE | ascii
174 | `"noise_comp_ratio"` | String | 1 | Compression Ratio for noise samples8/4, 8/3, 8/2, or 8/8 | ascii
175 | `"spare_12"` | Spare | 1 | Spare | -
176 | `"beam_overlap"` | ULong | 4 | Number of slant range samples in beam overlap(1-2, 2-3, 3-4, 4-5) | -
177 | `"lines_per_burst"` | ULong | 5 | Number of lines per burst for this image 5 values for beams SS1 to SS5 in WS and GM modes.One value for AP mode, all others set to zero. | lines
178 | `"spare_13"` | Spare | 1 | Spare | -
179 | `"orbit_state_vectors.1.state_vect_time_1"` | MJD | 1 | Time of state vector (record 1) | MJD
180 | `"orbit_state_vectors.1.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 1) | 10 -2m
181 | `"orbit_state_vectors.1.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 1) | 10 -2m
182 | `"orbit_state_vectors.1.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 1) | 10 -2m
183 | `"orbit_state_vectors.1.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
184 | `"orbit_state_vectors.1.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
185 | `"orbit_state_vectors.1.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
186 | `"orbit_state_vectors.2.state_vect_time_1"` | MJD | 1 | Time of state vector (record 2) | MJD
187 | `"orbit_state_vectors.2.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 2) | 10 -2m
188 | `"orbit_state_vectors.2.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 2) | 10 -2m
189 | `"orbit_state_vectors.2.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 2) | 10 -2m
190 | `"orbit_state_vectors.2.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
191 | `"orbit_state_vectors.2.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
192 | `"orbit_state_vectors.2.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
193 | `"orbit_state_vectors.3.state_vect_time_1"` | MJD | 1 | Time of state vector (record 3) | MJD
194 | `"orbit_state_vectors.3.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 3) | 10 -2m
195 | `"orbit_state_vectors.3.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 3) | 10 -2m
196 | `"orbit_state_vectors.3.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 3) | 10 -2m
197 | `"orbit_state_vectors.3.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
198 | `"orbit_state_vectors.3.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
199 | `"orbit_state_vectors.3.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
200 | `"orbit_state_vectors.4.state_vect_time_1"` | MJD | 1 | Time of state vector (record 4) | MJD
201 | `"orbit_state_vectors.4.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 4) | 10 -2m
202 | `"orbit_state_vectors.4.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 4) | 10 -2m
203 | `"orbit_state_vectors.4.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 4) | 10 -2m
204 | `"orbit_state_vectors.4.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
205 | `"orbit_state_vectors.4.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
206 | `"orbit_state_vectors.4.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
207 | `"orbit_state_vectors.5.state_vect_time_1"` | MJD | 1 | Time of state vector (record 5) | MJD
208 | `"orbit_state_vectors.5.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 5) | 10 -2m
209 | `"orbit_state_vectors.5.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 5) | 10 -2m
210 | `"orbit_state_vectors.5.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 5) | 10 -2m
211 | `"orbit_state_vectors.5.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
212 | `"orbit_state_vectors.5.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
213 | `"orbit_state_vectors.5.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
214 | `"spare_14"` | Spare | 1 | Spare | -
215 | `"slant_range_time"` | Float | 1 | 2-way slant range time origin (t0) | ns
216 | `"dop_coef"` | Float | 5 | Doppler centroid coefficients as a function of slant range time: D0, D1, D2, D3, and D4.where Doppler Centroid = D0 + D1(tSR-t0) + D2(tSR-t0)2 + D3(tSR-t0)3 + D4(tSR-t0)4 | HzHz/sHz/s2Hz/s3Hz/s4
217 | `"dop_conf"` | Float | 1 | Doppler Centroid Confidence MeasureValue between 0 and 1, 0 = poorest confidence, 1= highest confidence | -
218 | `"spare_15"` | Spare | 1 | Spare | -
219 | `"chirp_width"` | Float | 1 | 3-dB pulse width of chirp replica cross-correlation function between extract chirp and nominal chirp | samples
220 | `"chirp_sidelobe"` | Float | 1 | First side lobe level of chirp replica cross-correlation function between reconstructed chirp and nominal chirp | dB
221 | `"chirp_islr"` | Float | 1 | ISLR of chirp replica cross-correlation function between reconstructed chirp and nominal chirp | dB
222 | `"chirp_peak_loc"` | Float | 1 | Peak location of cross-correlation function between reconstructed chirp and nominal chirp | samples
223 | `"chirp_power"` | Float | 1 | Chirp power | -
224 | `"elev_corr_factor"` | Float | 1 | Elevation gain correction scaling factor applied to range compressed samples | -
225 | `"spare_16"` | Spare | 1 | Spare | -
226 | `"cal_info.1.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 1) | -
227 | `"cal_info.1.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 1) | -
228 | `"cal_info.1.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 1) | -
229 | `"cal_info.1.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 1) | degrees
230 | `"cal_info.2.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 2) | -
231 | `"cal_info.2.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 2) | -
232 | `"cal_info.2.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 2) | -
233 | `"cal_info.2.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 2) | degrees
234 | `"cal_info.3.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 3) | -
235 | `"cal_info.3.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 3) | -
236 | `"cal_info.3.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 3) | -
237 | `"cal_info.3.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 3) | degrees
238 | `"cal_info.4.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 4) | -
239 | `"cal_info.4.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 4) | -
240 | `"cal_info.4.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 4) | -
241 | `"cal_info.4.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 4) | degrees
242 | `"cal_info.5.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 5) | -
243 | `"cal_info.5.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 5) | -
244 | `"cal_info.5.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 5) | -
245 | `"cal_info.5.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 5) | degrees
246 | `"cal_info.6.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 6) | -
247 | `"cal_info.6.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 6) | -
248 | `"cal_info.6.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 6) | -
249 | `"cal_info.6.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 6) | degrees
250 | `"cal_info.7.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 7) | -
251 | `"cal_info.7.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 7) | -
252 | `"cal_info.7.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 7) | -
253 | `"cal_info.7.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 7) | degrees
254 | `"cal_info.8.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 8) | -
255 | `"cal_info.8.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 8) | -
256 | `"cal_info.8.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 8) | -
257 | `"cal_info.8.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 8) | degrees
258 | `"cal_info.9.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 9) | -
259 | `"cal_info.9.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 9) | -
260 | `"cal_info.9.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 9) | -
261 | `"cal_info.9.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 9) | degrees
262 | `"cal_info.10.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 10) | -
263 | `"cal_info.10.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 10) | -
264 | `"cal_info.10.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 10) | -
265 | `"cal_info.10.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 10) | degrees
266 | `"cal_info.11.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 11) | -
267 | `"cal_info.11.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 11) | -
268 | `"cal_info.11.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 11) | -
269 | `"cal_info.11.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 11) | degrees
270 | `"cal_info.12.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 12) | -
271 | `"cal_info.12.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 12) | -
272 | `"cal_info.12.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 12) | -
273 | `"cal_info.12.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 12) | degrees
274 | `"cal_info.13.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 13) | -
275 | `"cal_info.13.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 13) | -
276 | `"cal_info.13.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 13) | -
277 | `"cal_info.13.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 13) | degrees
278 | `"cal_info.14.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 14) | -
279 | `"cal_info.14.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 14) | -
280 | `"cal_info.14.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 14) | -
281 | `"cal_info.14.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 14) | degrees
282 | `"cal_info.15.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 15) | -
283 | `"cal_info.15.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 15) | -
284 | `"cal_info.15.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 15) | -
285 | `"cal_info.15.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 15) | degrees
286 | `"cal_info.16.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 16) | -
287 | `"cal_info.16.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 16) | -
288 | `"cal_info.16.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 16) | -
289 | `"cal_info.16.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 16) | degrees
290 | `"cal_info.17.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 17) | -
291 | `"cal_info.17.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 17) | -
292 | `"cal_info.17.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 17) | -
293 | `"cal_info.17.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 17) | degrees
294 | `"cal_info.18.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 18) | -
295 | `"cal_info.18.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 18) | -
296 | `"cal_info.18.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 18) | -
297 | `"cal_info.18.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 18) | degrees
298 | `"cal_info.19.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 19) | -
299 | `"cal_info.19.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 19) | -
300 | `"cal_info.19.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 19) | -
301 | `"cal_info.19.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 19) | degrees
302 | `"cal_info.20.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 20) | -
303 | `"cal_info.20.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 20) | -
304 | `"cal_info.20.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 20) | -
305 | `"cal_info.20.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 20) | degrees
306 | `"cal_info.21.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 21) | -
307 | `"cal_info.21.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 21) | -
308 | `"cal_info.21.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 21) | -
309 | `"cal_info.21.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 21) | degrees
310 | `"cal_info.22.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 22) | -
311 | `"cal_info.22.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 22) | -
312 | `"cal_info.22.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 22) | -
313 | `"cal_info.22.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 22) | degrees
314 | `"cal_info.23.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 23) | -
315 | `"cal_info.23.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 23) | -
316 | `"cal_info.23.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 23) | -
317 | `"cal_info.23.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 23) | degrees
318 | `"cal_info.24.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 24) | -
319 | `"cal_info.24.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 24) | -
320 | `"cal_info.24.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 24) | -
321 | `"cal_info.24.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 24) | degrees
322 | `"cal_info.25.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 25) | -
323 | `"cal_info.25.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 25) | -
324 | `"cal_info.25.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 25) | -
325 | `"cal_info.25.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 25) | degrees
326 | `"cal_info.26.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 26) | -
327 | `"cal_info.26.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 26) | -
328 | `"cal_info.26.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 26) | -
329 | `"cal_info.26.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 26) | degrees
330 | `"cal_info.27.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 27) | -
331 | `"cal_info.27.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 27) | -
332 | `"cal_info.27.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 27) | -
333 | `"cal_info.27.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 27) | degrees
334 | `"cal_info.28.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 28) | -
335 | `"cal_info.28.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 28) | -
336 | `"cal_info.28.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 28) | -
337 | `"cal_info.28.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 28) | degrees
338 | `"cal_info.29.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 29) | -
339 | `"cal_info.29.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 29) | -
340 | `"cal_info.29.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 29) | -
341 | `"cal_info.29.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 29) | degrees
342 | `"cal_info.30.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 30) | -
343 | `"cal_info.30.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 30) | -
344 | `"cal_info.30.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 30) | -
345 | `"cal_info.30.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 30) | degrees
346 | `"cal_info.31.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 31) | -
347 | `"cal_info.31.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 31) | -
348 | `"cal_info.31.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 31) | -
349 | `"cal_info.31.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 31) | degrees
350 | `"cal_info.32.max_cal"` | Float | 3 | Max of Cal pulses 1, 2, and 3 amplitude (record 32) | -
351 | `"cal_info.32.avg_cal"` | Float | 3 | Average of Cal pulse 1, 2, and 3 amplitude over the 3 dB on either side of the max amplitude (record 32) | -
352 | `"cal_info.32.avg_val_1a"` | Float | 1 | Average of Cal pulse 1A over the sample window (record 32) | -
353 | `"cal_info.32.phs_cal"` | Float | 4 | Extracted phase for calibration pulse 1, 1A, 2, and 3 (record 32) | degrees
354 | `"spare_17"` | Spare | 1 | Spare | -
355 | `"first_line_time"` | MJD | 1 | Zero Doppler Time at first line of imagette | MJD
356 | `"first_line_tie_points.range_samp_nums_first"` | ULong | 3 | Range sample number Gives the range location of the grid points. First range sample is 1, is M (includes zero filled samples) | -
357 | `"first_line_tie_points.slant_range_times_first"` | Float | 3 | 2 way slant range time to range sample | ns
358 | `"first_line_tie_points.inc_angles_first"` | Float | 3 | Incidence Angle at range sample | deg.
359 | `"first_line_tie_points.lats_first"` | SLong | 3 | geodetic latitude of range sample (positive north) | (1e-6) degrees
360 | `"first_line_tie_points.longs_first"` | SLong | 3 | geodetic longitude of range sample (positive east) | (1e-6) degrees
361 | `"mid_line_time"` | MJD | 1 | Zero Doppler Time at centre line of imagette | MJD
362 | `"mid_range_line_nums"` | ULong | 1 | Range line number of the center range line | -
363 | `"mid_line_tie_points.range_samp_nums_mid"` | ULong | 3 | Range sample number Gives the range location of the grid points. First range sample is 1, is M (includes zero filled samples) | -
364 | `"mid_line_tie_points.slant_range_times_mid"` | Float | 3 | 2 way slant range time to range sample | ns
365 | `"mid_line_tie_points.inc_angles_mid"` | Float | 3 | Incidence Angle at range sample | deg.
366 | `"mid_line_tie_points.lats_mid"` | SLong | 3 | geodetic latitude of range sample (positive north) | (1e-6) degrees
367 | `"mid_line_tie_points.longs_mid"` | SLong | 3 | geodetic longitude of range sample (positive east) | (1e-6) degrees
368 | `"last_line_time"` | MJD | 1 | Zero Doppler Time at last line of imagette | MJD
369 | `"last_line_num"` | ULong | 1 | Range line number of the last range line | -
370 | `"last_line_tie_points.range_samp_nums_last"` | ULong | 3 | Range sample number Gives the range location of the grid points. First range sample is 1, is M (includes zero filled samples) | -
371 | `"last_line_tie_points.slant_range_times_last"` | Float | 3 | 2 way slant range time to range sample | ns
372 | `"last_line_tie_points.inc_angles_last"` | Float | 3 | Incidence Angle at range sample | deg.
373 | `"last_line_tie_points.lats_last"` | SLong | 3 | geodetic latitude of range sample (positive north) | (1e-6) degrees
374 | `"last_line_tie_points.longs_last"` | SLong | 3 | geodetic longitude of range sample (positive east) | (1e-6) degrees
375 | `"swst_offset"` | Float | 1 | Wave cell SWST offset from center of the sub-swath to start of imagette. 208 ns increments | ns
376 | `"ground_range_bias"` | Float | 1 | Wave cell Ground range bias from centre of the Sub-Swath to the centre of the imagette (Ground range, km) | km
377 | `"elev_angle_bias"` | Float | 1 | Wave cell Elevation angle biasfrom centre of the Sub-Swath elevation to the centre of the imagette (deg) | deg
378 | `"imagette_range_len"` | Float | 1 | Imagette length in range (m) | m
379 | `"imagette_az_len"` | Float | 1 | Imagette length in azimuth (m) | m
380 | `"imagette_range_res"` | Float | 1 | Nominal Imagette resolution in slant range (m) | m
381 | `"ground_res"` | Float | 1 | Nominal resolution in ground range | m
382 | `"imagette_az_res"` | Float | 1 | Nominal Imagette resolution in azimuth (m) | m
383 | `"platform_alt"` | Float | 1 | Altitude (platform to ellipsoid) in metres (centre of wave cell) | m
384 | `"platform_vel"` | Float | 1 | Platform Velocity (m/s)w.r.t moving earth | m/s
385 | `"slant_range"` | Float | 1 | Range to centre of imagette (m)from platform to target | m
386 | `"cw_drift"` | Float | 1 | CW signal drift | -
387 | `"wave_subcycle"` | UShort | 1 | Wave sub-cycle (1 or 2) of this wave cell | -
388 | `"earth_radius"` | Float | 1 | Earth Radius at imagette center sample | m
389 | `"sat_height"` | Float | 1 | Satellite distance to earth center | m
390 | `"first_sample_slant_range"` | Float | 1 | Distance from satellite to first range pixel in the full SLC image | m
391 | `"spare_18"` | Spare | 1 | Spare | -
392 | `"elevation_pattern.slant_range_time"` | Float | 11 | 2 way slant range times | ns
393 | `"elevation_pattern.elevation_angles"` | Float | 11 | Corresponding elevation angles | degrees
394 | `"elevation_pattern.antenna_pattern"` | Float | 11 | Corresponding two-way antenna elevation pattern values | dB
395 | `"spare_19"` | Spare | 1 | Spare | -