Supported ENVISAT Products |

## 10-arcminute mds

Fields of ENVISAT ATS_MET_2P_meteo_user_prod Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"dsr_time"` | MJD | 1 | Nadir UTC time in MJD format | MJD
1 | `"rec_qua_ind"` | SChar | 1 | Record Quality indicator | -
2 | `"spare_1"` | Spare | 1 | Spare | -
3 | `"lat"` | SLong | 1 | Latitude of 10 arcmin cell | (1e-6) degrees
4 | `"lon"` | SLong | 1 | Longitude of 10 arcmin cell | (1e-6) degrees
5 | `"sa_12bt_clr_nad"` | SLong | 1 | Nadir spatially averaged 12 micron BT of all clear pixels 10 arcmin cells | K/1000
6 | `"sa_11bt_clr_nad"` | SLong | 1 | Nadir spatially averaged 11 micron BT of all clear pixels in 10 arcmin cells | K/1000
7 | `"sa_37bt_clr_nad"` | SLong | 1 | Nadir spatially averaged 3.7 micron BT of all clear pixels in 10 arcmin cells | K/1000
8 | `"sa_12bt_clr_for"` | SLong | 1 | Forward spatially averaged 12 micron BT of all clear pixels in 10 arcmin cells | K/1000
9 | `"sa_11bt_clr_for"` | SLong | 1 | Forward spatially averaged 11 micron BT of all clear pixels in 10 arcmin cells | K/1000
10 | `"sa_37bt_clr_for"` | SLong | 1 | Forward spatially averaged 3.7 micron BT of all clear pixels in 10 arcmin cells | K/1000
11 | `"m_actrk_pix_num"` | SShort | 1 | Mean across-track pixel number | none
12 | `"m_nad"` | SShort | 1 | Mean nadir-only SST 10 arcmin cells | K/100
13 | `"pix_nad"` | UShort | 1 | Number of pixels in nadir-only average, 10 arcmin cells | none
14 | `"m_dual_vw"` | SShort | 1 | Mean dual-view SST in 10 arcmin cells | K/100
15 | `"pix_dual_vw"` | UShort | 1 | Number of pixels in dual-view average, 10 arcmin cells | none
16 | `"ast_conf_flags"` | UShort | 2 | AST confidence word | flags