update_luts |

### update_luts

Retrieve latest lookup tables for specified sensor.

Location
Details
Command Line Usage

#### Location

SeaDAS-Toolbox -> update_luts

#### Details

update_luts retrieves latest lookup tables for specified sensor.

update_luts GUI

Arguments/Keywords

UI Element Name | Type | Description | Required/Optional | Default Value
| aqua | boolean | install MODIS Aqua files | Optional | true
terra | boolean | install MODIS Terra files | Optional | true
seawifs | boolean | install SeaWIFS files | Optional | true
viirsn | boolean | install VIIRS SNPP files | Optional | true
viirsj1 | boolean | install VIIRS JPSS1 files | Optional | true
viirsj2 | boolean | install VIIRS JPSS2 files | Optional | true

Actions/Buttons

UI Element Name | Type | Description
Run | Button | Executes the update_luts command with arguments provided in the UI.
Cancel | Button | Closes current processor GUI.
Apply | Button | Makes current arguments effective.
? | Button | Displays the help content of the current command.

#### Command Line Usage

    usage: update_luts [-h] [-e] [-v] [-n] [--timeout TIMEOUT] [--version] MISSION

    Retrieve latest lookup tables for specified sensor.

    positional arguments:
      MISSION            sensor or platform to process; one of:
                         all, common, seawifs, hico, modisa, modist, viirsn, viirsj1, viirsj2, oci, aqua, terra, npp, j1, j2

    options:
      -h, --help         show this help message and exit
      -e, --eval         also download evaluation LUTs (default: False)
      -v, --verbose      print status messages (default: 0)
      -n, --dry-run      no action; preview files to be downloaded (default: False)
      --timeout TIMEOUT  network timeout in seconds (default: 10)
      --version          show program's version number and exit