Supported ENVISAT Products |

## Scan pixel x and y ADS

Fields of ENVISAT ATS_TOA_1P_ADSR_scan Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"dsr_time"` | MJD | 1 | Scan UTC time in MJD format | MJD
1 | `"attach_flag"` | UChar | 1 | Attachment Flag (always set to zero for this ADS) | flag
2 | `"spare_1"` | Spare | 1 | Spare | -
3 | `"instr_scan_num"` | UShort | 1 | instrument scan number | -
4 | `"tie_pix_x"` | SLong | 99 | tie pixel x coordinate | m
5 | `"tie_pix_y"` | SLong | 99 | tie pixel y coordinate | m
6 | `"spare_2"` | Spare | 1 | spare | -