Supported ENVISAT Products |

INDEX BANDS PRODUCTS

## AATSR TOA Level 1b Confidence Flag Codings

Flags of ENVISAT ATS_TOA_1P_confid_flags Products

Identifier | Bit Index | Description
`"BLANKING"` | 0 | Blanking Pulse
`"COSMETIC"` | 1 | Cosmetic Fill Pixel
`"SCAN_ABSENT"` | 2 | Entire scan absent from telemetry
`"ABSENT"` | 3 | Pixel absent from telemetry
`"NOT_DECOMPR"` | 4 | Pixel not decompressed owing to error in packet validation
`"NO_SIGNAL"` | 5 | No signal in some channel (zero count)
`"SATURATION"` | 6 | Saturation in some channel (maximum count)
`"OUT_OF_RANGE"` | 7 | Derived radiance of some channel outside range of calibration
`"NO_CALIB_PARAM"` | 8 | Calibration Parameters unavailable for pixel
`"UNFILLED"` | 9 | Pixel unfilled (cosmetic fill algorithm unable to find nearest neighbour pixel)