C2RCC SeaWiFS Processing Parameters |

### SeaWiFS Processing Parameters

- Valid-pixel expression
  The arithmetic expression defines the pixels which are valid for processing. Pixels which are not valid will be marked as no-data in the target product.
- Salinity
  The value used as water salinity for the scene.
- Temperature
  The value used as water temperature for the scene.
- Ozone
  The value used as ozone if not provided by auxiliary data
- Air Pressure
  The surface air pressure at sea level if not provided by auxiliary data
- Output AC reflectances as rrs instead of rhow
  Reflectance values in the target product shall be written as remote sensing reflectances and not as water leaving reflectances
- Output TOSA reflectances
  Can be enabled to include the TOSA reflectances in the target product.