Supported ENVISAT Products |

## Main Processing parameters

Fields of ENVISAT ASAR_Main_ADSR Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"first_zero_doppler_time"` | MJD | 1 | First Zero Doppler Azimuth time of MDS which this data set describes Time of first range line in the MDS described by this data set. | MJD
1 | `"attach_flag"` | UChar | 1 | Attachment Flag (always set to zero for this ADSR) | flag
2 | `"last_zero_doppler_time"` | MJD | 1 | Last Zero Doppler Azimuth time of MDS which this data set describes Time of last range line in the MDS described by this data set | MJD
3 | `"work_order_id"` | String | 1 | Work Order ID (left-justified) | ascii
4 | `"time_diff"` | Float | 1 | Time difference between sensing time of first input line and zero Doppler time of first output image line (tdelta). (TBC)May be used during child product extraction from a stripline product (TBC). Left blank (set to zero) for non-stripline products. | s
5 | `"swath_id"` | String | 1 | Swath number IS1, IS2, IS3, IS4, IS5, IS6, or IS7 for IM, WV and AP modes.Set to WSØ for WS and GM modes | ascii
6 | `"range_spacing"` | Float | 1 | Range sample spacing | m
7 | `"azimuth_spacing"` | Float | 1 | Azimuth sample spacing at image center | m
8 | `"line_time_interval"` | Float | 1 | Azimuth sample spacing in time (Line Time Interval) | s
9 | `"num_output_lines"` | ULong | 1 | Number of output range lines in the image described by this ADS | lines
10 | `"num_samples_per_line"` | ULong | 1 | Number of samples per output range line (includes zero filled samples) | samples
11 | `"data_type"` | String | 1 | Output data type. SWORD, UWORD, or UBYTE | ascii
12 | `"spare_1"` | Spare | 1 | Spare | -
13 | `"data_analysis_flag"` | UChar | 1 | Raw Data Analysis used for Raw Data Correction. 0 = correction done using default parameters. 1 = correction done using raw data analysis results. | flag
14 | `"ant_elev_corr_flag"` | UChar | 1 | Antenna Elevation Pattern Correction Applied. 0 = no correction applied. 1 = correction applied. | flag
15 | `"chirp_extract_flag"` | UChar | 1 | Reconstructed Chirp used. 0 = nominal chirp replica used. 1 = reconstructed chirp used. | flag
16 | `"srgr_flag"` | UChar | 1 | Slant Range to Ground Range Conversion Applied. 0 = no conversion applied. 1 = conversion applied | flag
17 | `"dop_cen_flag"` | UChar | 1 | Doppler Centroid Estimation Performed. 0 = no estimation done. 1 = estimation done. | flag
18 | `"dop_amb_flag"` | UChar | 1 | Doppler Ambiguity Estimation Performed. 0 = no estimate done. 1 = estimate done | flag
19 | `"range_spread_comp_flag"` | UChar | 1 | Range-spreading loss compensation Applied. 0 = no compensation applied. 1 = compensation applied. | flag
20 | `"detected_flag"` | UChar | 1 | Detection Applied. 0 = output product is complex. 1 = output product was detected. | flag
21 | `"look_sum_flag"` | UChar | 1 | Look Summation Performed. 0 = product is single look. 1 = product is multi-looked. | flag
22 | `"rms_equal_flag"` | UChar | 1 | RMS Equalization performed. 0= rms equalization not performed during FBAQ decoding. 1 = rms equalization performed during FBAQ decoding. | flag
23 | `"ant_scal_flag"` | UChar | 1 | Antenna Elevation Gain Scaling Factor Applied. 0= no scaling factor applied. 1 = scaling factor applied. | flag
24 | `"vga_com_echo_flag"` | UChar | 1 | Receive Gain Droop Compensation Applied to Echo Data. 0 = no compensation applied. 1 = compensation applied. | flag
25 | `"vga_com_pulse_2_flag"` | UChar | 1 | Receive Gain Droop Compensation Applied Calibration Pulse P2. 0 = no compensation applied. 1 = compensation applied. | flag
26 | `"vga_com_pulse_zero_flag"` | UChar | 1 | Receive Gain Droop Compensation Applied Calibration Pulse P2 Order Zero: Nominal Time Delay Applied. 0 = no compensation applied. 1 = compensation applied. | flag
27 | `"inv_filt_comp_flag"` | UChar | 1 | Inverse FIlter used for range compression (GM Mode only). 0 = matched filter used for range compression. 1 = inverse filter used for range compression | flag
28 | `"spare_2"` | Spare | 1 | Spare | -
29 | `"raw_data_analysis.1.num_gaps"` | ULong | 1 | Number of input data gaps (a gap is defined as a predetermined number of range lines) (record 1) | gaps
30 | `"raw_data_analysis.1.num_missing_lines"` | ULong | 1 | Number of missing lines, excluding data gaps (record 1) | lines
31 | `"raw_data_analysis.1.range_samp_skip"` | ULong | 1 | Range sample skipping factor for raw data analysis (record 1) | samples
32 | `"raw_data_analysis.1.range_lines_skip"` | ULong | 1 | Range lines skipping factor for raw data analysis (record 1) | lines
33 | `"raw_data_analysis.1.calc_i_bias"` | Float | 1 | Calculated I channel bias (record 1) | -
34 | `"raw_data_analysis.1.calc_q_bias"` | Float | 1 | Calculated Q channel bias (record 1) | -
35 | `"raw_data_analysis.1.calc_i_std_dev"` | Float | 1 | Calculated I channel standard deviation (record 1) | -
36 | `"raw_data_analysis.1.calc_q_std_dev"` | Float | 1 | Calculated Q channel standard deviation (record 1) | -
37 | `"raw_data_analysis.1.calc_gain"` | Float | 1 | Calculated I/Q gain imbalance (record 1) | -
38 | `"raw_data_analysis.1.calc_quad"` | Float | 1 | Calculated I/Q quadrature departure (record 1) | -
39 | `"raw_data_analysis.1.i_bias_max"` | Float | 1 | I bias upper bound (record 1) | -
40 | `"raw_data_analysis.1.i_bias_min"` | Float | 1 | I bias lower bound (record 1) | -
41 | `"raw_data_analysis.1.q_bias_max"` | Float | 1 | Q bias upper bound (record 1) | -
42 | `"raw_data_analysis.1.q_bias_min"` | Float | 1 | Q bias lower bound (record 1) | -
43 | `"raw_data_analysis.1.gain_min"` | Float | 1 | I/Q gain lower bound (record 1) | -
44 | `"raw_data_analysis.1.gain_max"` | Float | 1 | I/Q gain upper bound (record 1) | -
45 | `"raw_data_analysis.1.quad_min"` | Float | 1 | I/Q quadrature departure lower bound (record 1) | -
46 | `"raw_data_analysis.1.quad_max"` | Float | 1 | I/Q quadrature departure upper bound (record 1) | -
47 | `"raw_data_analysis.1.i_bias_flag"` | UChar | 1 | I bias significance. 0 = I bias falls within acceptable range. 1 = I bias falls outside acceptable range (record 1) | flag
48 | `"raw_data_analysis.1.q_bias_flag"` | UChar | 1 | Q bias Significance. 0 = Q bias falls within acceptable range. 1 = Q bias falls outside acceptable range (record 1) | flag
49 | `"raw_data_analysis.1.gain_flag"` | UChar | 1 | I/Q Gain Significance. 0 = Gain falls within acceptable range. 1 = Gain falls outside acceptable range (record 1) | flag
50 | `"raw_data_analysis.1.quad_flag"` | UChar | 1 | I/Q Quadrature Departure Significance. 0 = Quadrature departure falls within acceptable range. 1 =Quadrature departure falls outside acceptable range (record 1) | flag
51 | `"raw_data_analysis.1.used_i_bias"` | Float | 1 | I channel bias used for correction (may be different from measured value) (record 1) | -
52 | `"raw_data_analysis.1.used_q_bias"` | Float | 1 | Q channel bias used for correction (may be different from measured value) (record 1) | -
53 | `"raw_data_analysis.1.used_gain"` | Float | 1 | I/Q gain imbalance used for correction (may be different from measured value) (record 1) | -
54 | `"raw_data_analysis.1.used_quad"` | Float | 1 | I/Q quadrature departure used for correction (may be different from measured value) (record 1) | -
55 | `"raw_data_analysis.2.num_gaps"` | ULong | 1 | Number of input data gaps (a gap is defined as a predetermined number of range lines) (record 2) | gaps
56 | `"raw_data_analysis.2.num_missing_lines"` | ULong | 1 | Number of missing lines, excluding data gaps (record 2) | lines
57 | `"raw_data_analysis.2.range_samp_skip"` | ULong | 1 | Range sample skipping factor for raw data analysis (record 2) | samples
58 | `"raw_data_analysis.2.range_lines_skip"` | ULong | 1 | Range lines skipping factor for raw data analysis (record 2) | lines
59 | `"raw_data_analysis.2.calc_i_bias"` | Float | 1 | Calculated I channel bias (record 2) | -
60 | `"raw_data_analysis.2.calc_q_bias"` | Float | 1 | Calculated Q channel bias (record 2) | -
61 | `"raw_data_analysis.2.calc_i_std_dev"` | Float | 1 | Calculated I channel standard deviation (record 2) | -
62 | `"raw_data_analysis.2.calc_q_std_dev"` | Float | 1 | Calculated Q channel standard deviation (record 2) | -
63 | `"raw_data_analysis.2.calc_gain"` | Float | 1 | Calculated I/Q gain imbalance (record 2) | -
64 | `"raw_data_analysis.2.calc_quad"` | Float | 1 | Calculated I/Q quadrature departure (record 2) | -
65 | `"raw_data_analysis.2.i_bias_max"` | Float | 1 | I bias upper bound (record 2) | -
66 | `"raw_data_analysis.2.i_bias_min"` | Float | 1 | I bias lower bound (record 2) | -
67 | `"raw_data_analysis.2.q_bias_max"` | Float | 1 | Q bias upper bound (record 2) | -
68 | `"raw_data_analysis.2.q_bias_min"` | Float | 1 | Q bias lower bound (record 2) | -
69 | `"raw_data_analysis.2.gain_min"` | Float | 1 | I/Q gain lower bound (record 2) | -
70 | `"raw_data_analysis.2.gain_max"` | Float | 1 | I/Q gain upper bound (record 2) | -
71 | `"raw_data_analysis.2.quad_min"` | Float | 1 | I/Q quadrature departure lower bound (record 2) | -
72 | `"raw_data_analysis.2.quad_max"` | Float | 1 | I/Q quadrature departure upper bound (record 2) | -
73 | `"raw_data_analysis.2.i_bias_flag"` | UChar | 1 | I bias significance. 0 = I bias falls within acceptable range. 1 = I bias falls outside acceptable range (record 2) | flag
74 | `"raw_data_analysis.2.q_bias_flag"` | UChar | 1 | Q bias Significance. 0 = Q bias falls within acceptable range. 1 = Q bias falls outside acceptable range (record 2) | flag
75 | `"raw_data_analysis.2.gain_flag"` | UChar | 1 | I/Q Gain Significance. 0 = Gain falls within acceptable range. 1 = Gain falls outside acceptable range (record 2) | flag
76 | `"raw_data_analysis.2.quad_flag"` | UChar | 1 | I/Q Quadrature Departure Significance. 0 = Quadrature departure falls within acceptable range. 1 =Quadrature departure falls outside acceptable range (record 2) | flag
77 | `"raw_data_analysis.2.used_i_bias"` | Float | 1 | I channel bias used for correction (may be different from measured value) (record 2) | -
78 | `"raw_data_analysis.2.used_q_bias"` | Float | 1 | Q channel bias used for correction (may be different from measured value) (record 2) | -
79 | `"raw_data_analysis.2.used_gain"` | Float | 1 | I/Q gain imbalance used for correction (may be different from measured value) (record 2) | -
80 | `"raw_data_analysis.2.used_quad"` | Float | 1 | I/Q quadrature departure used for correction (may be different from measured value) (record 2) | -
81 | `"spare_3"` | Spare | 1 | Spare | -
82 | `"start_time.1.first_obt"` | ULong | 2 | On-board binary time of first input line processed. LSB accurate to 15.26 us. (Contained in two long integers) (record 1) | -
83 | `"start_time.1.first_mjd"` | MJD | 1 | Sensing time (MJD format) of first input line processed converted from satellite binary time (record 1) | MJD
84 | `"start_time.2.first_obt"` | ULong | 2 | On-board binary time of first input line processed. LSB accurate to 15.26 us. (Contained in two long integers) (record 2) | -
85 | `"start_time.2.first_mjd"` | MJD | 1 | Sensing time (MJD format) of first input line processed converted from satellite binary time (record 2) | MJD
86 | `"parameter_codes.first_swst_code"` | UShort | 5 | Sampling Window Start time code of first processed line | code
87 | `"parameter_codes.last_swst_code"` | UShort | 5 | Sampling Window Start time code of last processed line | code
88 | `"parameter_codes.pri_code"` | UShort | 5 | Pulse Repetition Interval code | code
89 | `"parameter_codes.tx_pulse_len_code"` | UShort | 5 | Tx pulse length | code
90 | `"parameter_codes.tx_bw_code"` | UShort | 5 | Tx pulse bandwidth | code
91 | `"parameter_codes.echo_win_len_code"` | UShort | 5 | Echo Window Length | code
92 | `"parameter_codes.up_code"` | UShort | 5 | Upconverter Level - Upconverter gain set on the instrument | code
93 | `"parameter_codes.down_code"` | UShort | 5 | Downconverter Level - Downconverter gain set on the instrument | code
94 | `"parameter_codes.resamp_code"` | UShort | 5 | Resampling factor for echo data | code
95 | `"parameter_codes.beam_adj_code"` | UShort | 5 | Beam adjustment delta | code
96 | `"parameter_codes.beam_set_num_code"` | UShort | 5 | Antenna Beam Set Number | code
97 | `"parameter_codes.tx_monitor_code"` | UShort | 5 | Auxiliary Tx Monitor Level | code
98 | `"spare_4"` | Spare | 1 | Spare | -
99 | `"error_counters.num_err_swst"` | ULong | 1 | Number of errors detected in Sampling Window start time field. | -
100 | `"error_counters.num_err_pri"` | ULong | 1 | Number of errors detected in PRI code field | -
101 | `"error_counters.num_err_tx_pulse_len"` | ULong | 1 | Number of errors detected in Tx pulse length field | -
102 | `"error_counters.num_err_tx_pulse_bw"` | ULong | 1 | Number of errors detected in Tx pulse bandwidth field. | -
103 | `"error_counters.num_err_echo_win_len"` | ULong | 1 | Number of errors detected in Echo Window Length field. | -
104 | `"error_counters.num_err_up"` | ULong | 1 | Number of errors detected in Upconverter Level field. | -
105 | `"error_counters.num_err_down"` | ULong | 1 | Number of errors detected in Downconverter Level field. | -
106 | `"error_counters.num_err_resamp"` | ULong | 1 | Number of errors detected in Resampling factor for echo data field. | -
107 | `"error_counters.num_err_beam_adj"` | ULong | 1 | Number of errors detected in Beam adjustment delta field. | -
108 | `"error_counters.num_err_beam_set_num"` | ULong | 1 | Number of errors detected in Antenna Beam Set Number field. | -
109 | `"spare_5"` | Spare | 1 | Spare | -
110 | `"image_parameters.first_swst_value"` | Float | 5 | Sampling Window Start time of first processed line | s
111 | `"image_parameters.last_swst_value"` | Float | 5 | Sampling Window Start time of last processed line | s
112 | `"image_parameters.swst_changes"` | ULong | 5 | Number of Sample Window Start Time changes within a beam | -
113 | `"image_parameters.prf_value"` | Float | 5 | Pulse Repetition Frequency | Hz
114 | `"image_parameters.tx_pulse_len_value"` | Float | 5 | Tx pulse length | s
115 | `"image_parameters.tx_pulse_bw_value"` | Float | 5 | Tx pulse bandwidth | Hz
116 | `"image_parameters.echo_win_len_value"` | Float | 5 | Echo Window Length | s
117 | `"image_parameters.up_value"` | Float | 5 | Upconverter Level - Upconverter gain set on the instrument | dB
118 | `"image_parameters.down_value"` | Float | 5 | Downconverter Level - Downconverter gain set on the instrument | dB
119 | `"image_parameters.resamp_value"` | Float | 5 | Resampling factor | -
120 | `"image_parameters.beam_adj_value"` | Float | 5 | Beam adjustment delta | deg.
121 | `"image_parameters.beam_set_value"` | UShort | 5 | Antenna Beam Set Number | -
122 | `"image_parameters.tx_monitor_value"` | Float | 5 | Auxiliary Tx Monitor Level | -
123 | `"spare_6"` | Spare | 1 | Spare | -
124 | `"first_proc_range_samp"` | ULong | 1 | First processed input range sample, first sample is 1 | samples
125 | `"range_ref"` | Float | 1 | Range spreading loss reference range | m
126 | `"range_samp_rate"` | Float | 1 | Range sampling rate | Hz
127 | `"radar_freq"` | Float | 1 | Radar Frequency | Hz
128 | `"num_looks_range"` | UShort | 1 | Number of range looks | looks
129 | `"filter_window"` | String | 1 | Matched filter window type:HAMMING or KAISERØ or NONEØØØ | ascii
130 | `"window_coef_range"` | Float | 1 | Window coefficient for range-matched filter | -
131 | `"bandwidth.look_bw_range"` | Float | 5 | Range Look Bandwidth (null to null) | Hz
132 | `"bandwidth.tot_bw_range"` | Float | 5 | Total processed range bandwidth (null to null) | Hz
133 | `"nominal_chirp.1.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 1) | -, s-1, s-2, s-3
134 | `"nominal_chirp.1.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 1) | cycles,Hz,Hz/s,Hz/s2
135 | `"nominal_chirp.2.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 2) | -, s-1, s-2, s-3
136 | `"nominal_chirp.2.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 2) | cycles,Hz,Hz/s,Hz/s2
137 | `"nominal_chirp.3.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 3) | -, s-1, s-2, s-3
138 | `"nominal_chirp.3.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 3) | cycles,Hz,Hz/s,Hz/s2
139 | `"nominal_chirp.4.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 4) | -, s-1, s-2, s-3
140 | `"nominal_chirp.4.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 4) | cycles,Hz,Hz/s,Hz/s2
141 | `"nominal_chirp.5.nom_chirp_amp"` | Float | 4 | 4 nominal chirp amplitude coefficients (record 5) | -, s-1, s-2, s-3
142 | `"nominal_chirp.5.nom_chirp_phs"` | Float | 4 | 4 nominal chirp phase coefficients (record 5) | cycles,Hz,Hz/s,Hz/s2
143 | `"spare_7"` | Spare | 1 | Spare | -
144 | `"num_lines_proc"` | ULong | 1 | Number of input lines processed | lines
145 | `"num_look_az"` | UShort | 1 | Number of Azimuth Looks | looks
146 | `"look_bw_az"` | Float | 1 | Azimuth Look Bandwidth (null to null) -- this is the nominal value only for GM, WS, and AP. | Hz
147 | `"to_bw_az"` | Float | 1 | Processed Azimuth bandwidth (null to null) -- this field is used only for IM products and WV imagettes. Filled with zeros otherwise. | Hz
148 | `"filter_az"` | String | 1 | Matched filter window type:HAMMING or KAISERØ or NONEØØØ | ascii
149 | `"filter_coef_az"` | Float | 1 | Window coefficient for azimuth-matched filter | -
150 | `"az_fm_rate"` | Float | 3 | 3 co-efficients for Azimuth FM rate: Azimuth FM rate = C0 + C1(tSR-t0) + C2(tSR - t0)2tSR = 2 way slant range time | Hz/sHz/s2Hz/s3
151 | `"ax_fm_origin"` | Float | 1 | 2 way slant range time origin (t0) for Azimuth FM rate calculation | ns
152 | `"dop_amb_conf"` | Float | 1 | Doppler Centroid Ambiguity Confidence Measure. Value between 0 and 1, 0 = poorest confidence, 1= highest confidence | -
153 | `"spare_8"` | Spare | 1 | Spare | -
154 | `"calibration_factors.1.proc_scaling_fact"` | Float | 1 | Processor scaling factor (factor units are linear when using Range/Doppler algorithm, dB when Specan is used) (record 1) | -
155 | `"calibration_factors.1.ext_cal_fact"` | Float | 1 | External Calibration Scaling Factor (mode/swath/polarization dependent) (record 1) | -
156 | `"calibration_factors.2.proc_scaling_fact"` | Float | 1 | Processor scaling factor (factor units are linear when using Range/Doppler algorithm, dB when Specan is used) (record 2) | -
157 | `"calibration_factors.2.ext_cal_fact"` | Float | 1 | External Calibration Scaling Factor (mode/swath/polarization dependent) (record 2) | -
158 | `"noise_estimation.noise_power_corr"` | Float | 5 | Noise power correction factors | -
159 | `"noise_estimation.num_noise_lines"` | ULong | 5 | Number of noise lines used to calculate factors | -
160 | `"spare_9"` | Spare | 1 | Spare | -
161 | `"spare_10"` | Spare | 1 | Spare | -
162 | `"output_statistics.1.out_mean"` | Float | 1 | Output data mean. Magnitude for detected products, real sample mean for SLC products (record 1) | -
163 | `"output_statistics.1.out_imag_mean"` | Float | 1 | Output imaginary data mean. Used for SLC products only (set to zero otherwise) (record 1) | -
164 | `"output_statistics.1.out_std_dev"` | Float | 1 | Output data standard deviation. Magnitude std. dev. for detected products, real sample std. dev. for SLC products (record 1) | -
165 | `"output_statistics.1.out_imag_std_dev"` | Float | 1 | Output imaginary data standard deviation. Used for SLC products only (set to zero otherwise) (record 1) | -
166 | `"output_statistics.2.out_mean"` | Float | 1 | Output data mean. Magnitude for detected products, real sample mean for SLC products (record 2) | -
167 | `"output_statistics.2.out_imag_mean"` | Float | 1 | Output imaginary data mean. Used for SLC products only (set to zero otherwise) (record 2) | -
168 | `"output_statistics.2.out_std_dev"` | Float | 1 | Output data standard deviation. Magnitude std. dev. for detected products, real sample std. dev. for SLC products (record 2) | -
169 | `"output_statistics.2.out_imag_std_dev"` | Float | 1 | Output imaginary data standard deviation. Used for SLC products only (set to zero otherwise) (record 2) | -
170 | `"spare_11"` | Spare | 1 | Spare | -
171 | `"echo_comp"` | String | 1 | Compression Method used for echo samples. FBAQ, S&MØ, NONE | ascii
172 | `"echo_comp_ratio"` | String | 1 | Compression Ratio for echo samples. 8/4, 8/3, 8/2, or 8/8 | ascii
173 | `"init_cal_comp"` | String | 1 | Compression Method used for initial calibration samples. FBAQ, S&MØ, NONE | ascii
174 | `"init_cal_ratio"` | String | 1 | Compression Ratio for initial calibration samples. 8/4, 8/3, 8/2, or 8/8 | ascii
175 | `"per_cal_comp"` | String | 1 | Compression Method used for periodic calibration samples. FBAQ, S&MØ, NONE | ascii
176 | `"per_cal_ratio"` | String | 1 | Compression Ratio for periodic calibration samples. 8/4, 8/3, 8/2, or 8/8 | ascii
177 | `"noise_comp"` | String | 1 | Compression Method used for noise samples. FBAQ, S&MØ, NONE | ascii
178 | `"noise_comp_ratio"` | String | 1 | Compression Ratio for noise samples. 8/4, 8/3, 8/2, or 8/8 | ascii
179 | `"spare_12"` | Spare | 1 | Spare | -
180 | `"beam_merge_sl_range"` | ULong | 4 | Number of slant range samples in beam merging, one value per mergae rregion (1-2, 2-3, 3-4, 4-5) | -
181 | `"beam_merge_alg_param"` | Float | 4 | Beam merge algorithm parameter used for beam merging, one value per merge region (1-2, 2-3, 3-4. 4-5) | -
182 | `"lines_per_burst"` | ULong | 5 | Number of lines per burst for this image. 5 values for beams SS1 to SS5 in WS and GM modes. Two values for AP mode, all others set to zero. | lines
183 | `"spare_13"` | Spare | 1 | Spare | -
184 | `"orbit_state_vectors.1.state_vect_time_1"` | MJD | 1 | Time of state vector (record 1) | MJD
185 | `"orbit_state_vectors.1.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 1) | 10 -2m
186 | `"orbit_state_vectors.1.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 1) | 10 -2m
187 | `"orbit_state_vectors.1.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 1) | 10 -2m
188 | `"orbit_state_vectors.1.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
189 | `"orbit_state_vectors.1.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
190 | `"orbit_state_vectors.1.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 1) | 10 -5m/s
191 | `"orbit_state_vectors.2.state_vect_time_1"` | MJD | 1 | Time of state vector (record 2) | MJD
192 | `"orbit_state_vectors.2.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 2) | 10 -2m
193 | `"orbit_state_vectors.2.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 2) | 10 -2m
194 | `"orbit_state_vectors.2.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 2) | 10 -2m
195 | `"orbit_state_vectors.2.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
196 | `"orbit_state_vectors.2.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
197 | `"orbit_state_vectors.2.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 2) | 10 -5m/s
198 | `"orbit_state_vectors.3.state_vect_time_1"` | MJD | 1 | Time of state vector (record 3) | MJD
199 | `"orbit_state_vectors.3.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 3) | 10 -2m
200 | `"orbit_state_vectors.3.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 3) | 10 -2m
201 | `"orbit_state_vectors.3.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 3) | 10 -2m
202 | `"orbit_state_vectors.3.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
203 | `"orbit_state_vectors.3.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
204 | `"orbit_state_vectors.3.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 3) | 10 -5m/s
205 | `"orbit_state_vectors.4.state_vect_time_1"` | MJD | 1 | Time of state vector (record 4) | MJD
206 | `"orbit_state_vectors.4.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 4) | 10 -2m
207 | `"orbit_state_vectors.4.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 4) | 10 -2m
208 | `"orbit_state_vectors.4.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 4) | 10 -2m
209 | `"orbit_state_vectors.4.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
210 | `"orbit_state_vectors.4.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
211 | `"orbit_state_vectors.4.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 4) | 10 -5m/s
212 | `"orbit_state_vectors.5.state_vect_time_1"` | MJD | 1 | Time of state vector (record 5) | MJD
213 | `"orbit_state_vectors.5.x_pos_1"` | SLong | 1 | X position in Earth fixed reference frame (record 5) | 10 -2m
214 | `"orbit_state_vectors.5.y_pos_1"` | SLong | 1 | Y position in Earth fixed reference frame (record 5) | 10 -2m
215 | `"orbit_state_vectors.5.z_pos_1"` | SLong | 1 | Z position in Earth fixed reference frame (record 5) | 10 -2m
216 | `"orbit_state_vectors.5.x_vel_1"` | SLong | 1 | X velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
217 | `"orbit_state_vectors.5.y_vel_1"` | SLong | 1 | Y velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
218 | `"orbit_state_vectors.5.z_vel_1"` | SLong | 1 | Z velocity relative to Earth fixed reference frame (record 5) | 10 -5m/s
219 | `"spare_14"` | Spare | 1 | Spare | -