OLCI O2A Harmonisation Processor |

### Introduction

The OLCI O2A Harmonisation Processor provides a 'harmonisation' of OLCI bands 13-15, which are the new bands in the O2A absorption line (764.4 and 767.5 nm) and the existing channel at 761.25nm. This harmonisation provides a modification of the effective transmittances to their values which would be measured at their mean wavelengths and with nominal bandwidth.

OLCI O2A Harmonisation Algorithm Specification

OLCI O2A Harmonisation Processor Description

Command Line Processing