Supported ENVISAT Products |

INDEX PRODUCTS

## MERIS Level 1b Full Resolution Geophysical Product

Bands of ENVISAT MER_FR__1P_IODD5 Products

Tie-Point Grids of ENVISAT

Index | Identifier | Type | Description | Units | Bitmask
0 | `"latitude"` | Float | Latitude of the tie points (WGS-84), positive N | deg | n/a
1 | `"longitude"` | Float | Longitude of the tie points (WGS-84), Greenwich origin, positive E | deg | n/a
2 | `"dem_alt"` | Float | Digital elevation model altitude | m | n/a
3 | `"dem_rough"` | Float | Digital elevation model roughness | m | n/a
4 | `"lat_corr"` | Float | Digital elevation model latitude corrections | deg | n/a
5 | `"lon_corr"` | Float | Digital elevation model longitude corrections | deg | n/a
6 | `"sun_zenith"` | Float | Sun zenith angle | deg | n/a
7 | `"sun_azimuth"` | Float | Sun azimuth angles | deg | n/a
8 | `"view_zenith"` | Float | Viewing zenith angles | deg | n/a
9 | `"view_azimuth"` | Float | Viewing azimuth angles | deg | n/a
10 | `"zonal_wind"` | Float | Zonal wind | m/s | n/a
11 | `"merid_wind"` | Float | Meridional wind | m/s | n/a
12 | `"atm_press"` | Float | Mean sea level pressure | hPa | n/a
13 | `"ozone"` | Float | Total ozone | DU | n/a
14 | `"rel_hum"` | Float | Relative humidity | % | n/a

Bands of ENVISAT

Index | Identifier | Type | Description | Units | Bitmask
15 | `"radiance_1"` | Float | TOA radiance band 1 | mW/(m^2*sr*nm) | n/a
16 | `"radiance_2"` | Float | TOA radiance band 2 | mW/(m^2*sr*nm) | n/a
17 | `"radiance_3"` | Float | TOA radiance band 3 | mW/(m^2*sr*nm) | n/a
18 | `"radiance_4"` | Float | TOA radiance band 4 | mW/(m^2*sr*nm) | n/a
19 | `"radiance_5"` | Float | TOA radiance band 5 | mW/(m^2*sr*nm) | n/a
20 | `"radiance_6"` | Float | TOA radiance band 6 | mW/(m^2*sr*nm) | n/a
21 | `"radiance_7"` | Float | TOA radiance band 7 | mW/(m^2*sr*nm) | n/a
22 | `"radiance_8"` | Float | TOA radiance band 8 | mW/(m^2*sr*nm) | n/a
23 | `"radiance_9"` | Float | TOA radiance band 9 | mW/(m^2*sr*nm) | n/a
24 | `"radiance_10"` | Float | TOA radiance band 10 | mW/(m^2*sr*nm) | n/a
25 | `"radiance_11"` | Float | TOA radiance band 11 | mW/(m^2*sr*nm) | n/a
26 | `"radiance_12"` | Float | TOA radiance band 12 | mW/(m^2*sr*nm) | n/a
27 | `"radiance_13"` | Float | TOA radiance band 13 | mW/(m^2*sr*nm) | n/a
28 | `"radiance_14"` | Float | TOA radiance band 14 | mW/(m^2*sr*nm) | n/a
29 | `"radiance_15"` | Float | TOA radiance band 15 | mW/(m^2*sr*nm) | n/a
30 | `"l1_flags"` | UChar | Level 1b classification and quality flags | n/a | n/a
31 | `"ssi"` | UChar | Spectral shift index | n/a | n/a