Supported ENVISAT Products |

## Level 2 MDS(19) aerosol epsilon or cloud type and optical thickness

Fields of ENVISAT MER_RR__2P_MDSR_19_IODD6 Records

Index | Identifier | Field Type | Field Length | Description | Units
0 | `"dsr_time"` | MJD | 1 | Start Time of DSR | MJD
1 | `"quality_flag"` | UChar | 1 | Quality Indicator (-1 for blank MDSR, 0 otherwise) | flag
2 | `"air_cl_opt_pix"` | UChar | 2*sceneRasterWidth | Aerosol epsilon or cloud type and optical thickness pixels, interleaved by pixel | -